Marvell Serial ATA PCI-X Adapter RedHat Installation Disk README
----------------------------------------------------------------

This README file explains how to create a boot disk for RedHat 8 
and RedHat 9 based distributions.
The result of the process is a single boot disk that is suitable for both
RedHat 8 and RedHat 9 in UP/SMP and bigmem kernels.

Instructions -
--------------
1.. Create a directory where the kernel sources will be installed later on.
    For this README file, assume that the directory is /tmp/kernel_sources.

2.. Install RedHat 8 and 9 under the directory
    /tmp/kernel_sources/<kernel_version>.
    
    This installation will create two directories -
    /tmp/kernel_sources/2.4.18-14 and /tmp/kernel_sources/2.4.20-8
    
3.. Go to the RedHat directory in LinuxIAL within the driver's source files.

4.. Execute 'dos2unix gen_module.sh files/*'

5.. Execute 'sh gen_module.sh /tmp/kernel_sources'
    The gen_module.sh will scan all available kernels and will produce
    a boot diskette according to all kernel versions available in the
    /tmp/kernel_sources directory.

6.. The content of the 'files' directory is the boot diskette. Copy it to
    a diskette.

7.. Start the RedHat 8 or 9 installation on the require computer which
    Marvell Serial ATA adapter.

8.. During installation, select Expert Mode and follow the installation
    instruction. When a driver disk is requested, insert the boot diskette
    in drive A and continue the installation.
